VERSION:3 SOURCE_TIMESTAMP:4136BD21
NODE:I LEVEL:0 LINE:1 "D:\_Research\_AVR\hxRLCMetter\Firmware\src\usart.h"
NODE:I LEVEL:0 LINE:2 "C:\Program Files (x86)\CVAvr\inc\mega8.h"
NODE:F LEVEL:0 LINE:6 "USART_TransmitChar(unsigned char data)"
NODE:F LEVEL:0 LINE:17 "USART_TransmitBuf(unsigned char * data,int data_len)"
NODE:F LEVEL:0 LINE:30 "USART_HasData(void)"
NODE:F LEVEL:0 LINE:37 "USART_ReceiveChar(void)"
