VERSION:3 SOURCE_TIMESTAMP:423304CF
NODE:I LEVEL:0 LINE:11 "C:\Program Files (x86)\CVAVR\inc\mega8.h"
NODE:I LEVEL:0 LINE:13 "C:\Program Files (x86)\CVAVR\inc\string.h"
NODE:I LEVEL:0 LINE:14 "C:\Program Files (x86)\CVAVR\inc\stdint.h"
NODE:I LEVEL:0 LINE:15 "C:\Program Files (x86)\CVAVR\inc\stdbool.h"
NODE:I LEVEL:0 LINE:16 "C:\Program Files (x86)\CVAVR\inc\delay.h"
NODE:I LEVEL:0 LINE:17 "C:\Program Files (x86)\CVAVR\inc\stdio.h"
NODE:I LEVEL:0 LINE:19 "C:\Research\_AVR\hxRLCMetter\Firmware\src\lcd_d7225.h"
NODE:I LEVEL:0 LINE:20 "C:\Research\_AVR\hxRLCMetter\Firmware\src\usart.h"
NODE:M LEVEL:0 LINE:25 "LCD_CS_PORT"
NODE:M LEVEL:0 LINE:26 "LCD_DATA_PORT"
NODE:M LEVEL:0 LINE:27 "LCD_CLK_PORT"
NODE:M LEVEL:0 LINE:29 "POWER_HOLD"
NODE:M LEVEL:0 LINE:30 "C1EN"
NODE:M LEVEL:0 LINE:33 "OUT_M_C"
NODE:M LEVEL:0 LINE:34 "IN_M_C"
NODE:M LEVEL:0 LINE:35 "OUT_M_NR"
NODE:M LEVEL:0 LINE:36 "IN_M_NR"
NODE:M LEVEL:0 LINE:37 "OUT_M_NESR"
NODE:M LEVEL:0 LINE:38 "IN_M_NESR"
NODE:M LEVEL:0 LINE:40 "MODE_ESR"
NODE:M LEVEL:0 LINE:41 "MODE_C"
NODE:M LEVEL:0 LINE:42 "MODE_L"
NODE:M LEVEL:0 LINE:43 "MODE_R"
NODE:M LEVEL:0 LINE:44 "MODE_NONE"
NODE:M LEVEL:0 LINE:47 "MAX_IDLE"
NODE:M LEVEL:0 LINE:50 "MAX_WORKING"
NODE:M LEVEL:0 LINE:53 "AP_COUNT"
NODE:M LEVEL:0 LINE:56 "AP_THRESHOLD"
NODE:M LEVEL:0 LINE:58 "RCAL1_VAL"
NODE:M LEVEL:0 LINE:59 "RCAL2_VAL"
NODE:M LEVEL:0 LINE:60 "RCAL3_VAL"
NODE:M LEVEL:0 LINE:61 "RCAL4_VAL"
NODE:M LEVEL:0 LINE:62 "RCAL_RDSON"
NODE:M LEVEL:0 LINE:64 "RCAL1"
NODE:M LEVEL:0 LINE:65 "RCAL2"
NODE:M LEVEL:0 LINE:67 "RCAL3"
NODE:M LEVEL:0 LINE:68 "IN_RCAL3"
NODE:M LEVEL:0 LINE:69 "DDR_RCAL3"
NODE:M LEVEL:0 LINE:71 "RCAL4"
NODE:M LEVEL:0 LINE:72 "IN_RCAL4"
NODE:M LEVEL:0 LINE:73 "DDR_RCAL4"
NODE:M LEVEL:0 LINE:76 "CCAL"
NODE:M LEVEL:0 LINE:79 "LCAL"
NODE:M LEVEL:0 LINE:82 "CLOCK_FREQ"
NODE:M LEVEL:0 LINE:85 "PI"
NODE:M LEVEL:0 LINE:87 "R_ADC"
NODE:M LEVEL:0 LINE:89 "ESR1_ADC"
NODE:M LEVEL:0 LINE:90 "ESR2_ADC"
NODE:V LEVEL:0 LINE:96 "s_t0counter -> RAM:????"
NODE:V LEVEL:0 LINE:99 "s_t1counter -> RAM:????"
NODE:V LEVEL:0 LINE:102 "s_lastMode -> R5"
NODE:V LEVEL:0 LINE:105 "s_N0 -> EEPROM:????"
NODE:V LEVEL:0 LINE:108 "s_N1 -> EEPROM:????"
NODE:V LEVEL:0 LINE:111 "s_lastIdle -> RAM:????"
NODE:M LEVEL:0 LINE:116 "ESR2_MUL"
NODE:V LEVEL:0 LINE:119 "s_ESR1_Zero -> EEPROM:????"
NODE:V LEVEL:0 LINE:122 "s_ESR2_Zero -> EEPROM:????"
NODE:M LEVEL:0 LINE:125 "ESR_CAL_COUNT"
NODE:M LEVEL:0 LINE:129 "ESR_ADC_MAX"
NODE:V LEVEL:0 LINE:133 "s_ESR_ADC_CAL -> EEPROM:????"
NODE:C LEVEL:0 LINE:136 "s_ESR_CAL_R -> FLASH"
NODE:C LEVEL:0 LINE:140 "rcal -> FLASH"
NODE:V LEVEL:0 LINE:143 "s_R_Zero -> EEPROM:????"
NODE:V LEVEL:0 LINE:146 "s_bLowPower -> R4"
NODE:F LEVEL:0 LINE:155 "timer0_ovf_isr(void)"
NODE:F LEVEL:0 LINE:163 "timer1_ovf_isr(void)"
NODE:F LEVEL:0 LINE:170 "LCD_CS(uint8_t val)"
NODE:F LEVEL:0 LINE:177 "LCD_DATA(uint8_t val)"
NODE:F LEVEL:0 LINE:184 "LCD_CLK(uint8_t val)"
NODE:F LEVEL:0 LINE:193 "getTimer0Counter(void)"
NODE:F LEVEL:0 LINE:221 "getTimer1Counter(void)"
NODE:F LEVEL:0 LINE:248 "getMode(void)"
NODE:F LEVEL:0 LINE:271 "getModeStable(void)"
NODE:F LEVEL:0 LINE:305 "checkSetZero(void)"
NODE:F LEVEL:0 LINE:338 "powerOff(void)"
NODE:F LEVEL:0 LINE:347 "checkPowerOff(void)"
NODE:M LEVEL:0 LINE:375 "ADC_VREF_TYPE"
NODE:F LEVEL:0 LINE:378 "prepareADC(uint8_t adc_input)"
NODE:F LEVEL:0 LINE:387 "checkLowPower(void)"
NODE:F LEVEL:0 LINE:407 "configureHardware(void)"
NODE:F LEVEL:0 LINE:511 "disableCCal(void)"
NODE:F LEVEL:0 LINE:519 "enableCCal(void)"
NODE:F LEVEL:0 LINE:527 "disableOCR2(void)"
NODE:F LEVEL:0 LINE:534 "enableOCR2(void)"
NODE:F LEVEL:0 LINE:544 "countLC(void)"
NODE:F LEVEL:0 LINE:593 "readADC(void)"
NODE:F LEVEL:0 LINE:605 "readADC16_Sum(void)"
NODE:F LEVEL:0 LINE:620 "readADC16_Avg(void)"
NODE:F LEVEL:0 LINE:630 "calibrateLC(void)"
NODE:F LEVEL:0 LINE:645 "prepareMode(void)"
NODE:F LEVEL:0 LINE:664 "resetIdle(void)"
NODE:F LEVEL:0 LINE:671 "measureR(void)"
NODE:F LEVEL:0 LINE:795 "measureL(void)"
NODE:F LEVEL:0 LINE:840 "measureC(void)"
NODE:F LEVEL:0 LINE:886 "ESRInterpolate(uint16_t _esr_adc_val)"
NODE:F LEVEL:0 LINE:973 "GetESRADC(uint16_t * _pESR1Val,uint16_t * _pESR2Val,uint16_t * _pVal)"
NODE:F LEVEL:0 LINE:1018 "measureESR(void)"
NODE:F LEVEL:0 LINE:1058 "measure(void)"
NODE:F LEVEL:0 LINE:1160 "printESRCal(void)"
NODE:F LEVEL:0 LINE:1172 "checkDebugInput(void)"
NODE:F LEVEL:0 LINE:1228 "main(void)"
